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ABSTRACT
We introduce a peak mitigation technique for reference based systems that is similar to the tone reservation scheme employed in orthogonal frequency division multiplexing (OFDM) systems but without the cost in data rate. A comparison of reference-based systems under either peak or average power constraints is presented.
