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EXAMINATION ROOM GUIDE USING RFID FOR THE JUMBLING SYSTEM BASED EXAMS
ABSTRACT:

The main objective of this project is to develop an embedded system, which is used to verify and authenticate the authorized and display the room number.	
Radio-frequency identification (RFID) is a technology that uses radio waves to transfer data from an electronic tag, called RFID tag or label, attached to an object, through a reader for the purpose of identifying and tracking the object. Some RFID tags can be read from several meters away and beyond the line of sight of the reader. The application of bulk reading enables an almost-parallel reading of tags.
The tag's information is stored electronically. The RFID tag includes a small RF transmitter and receiver. An RFID reader transmits an encoded radio signal to interrogate the tag. The tag receives the message and responds with its identification information. Many RFID tags do not use a battery. Instead, the tag uses the radio energy transmitted by the reader as its energy source. The RFID system design includes a method of discriminating several tags that might be within the range of the RFID reader.
      Whenever the student enters into the Examination center, he has to keep his RFID TAG to the reader which is attached to our microcontroller based embedded board. And enters the password (if necessary, their roll number is password) through the keypad interfaced. At that moment the reader will checks weather the information of the student is correct or not and then it will decide to display the student room number on LCD display. If the information of the student is correct then he will be permitted inside otherwise he will not permit inside and switches on the buzzer. The information of the student will be send to the microcontroller through one wire protocol. And the information of the access system will be displayed on the LCD which we embedded to our board.

This project uses regulated 5v, 750ma power supply. 7805 three terminal voltage regulator is used for voltage regulation. Bridge type full wave rectifier is used to rectify the ac output of secondary of 230/18v step down transformer.
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SOFTWARE: 
1. Embedded ‘c’
1. Ride to write code
1. Isp to burn the chip
1. Keil compiler.                            
	
HARDWARE:
1. Atmel based our own developed board
1. Power supply
1. Rfid reader
1. Rfid tag
1. Key pad
1. Lcd display
1. Relay
1. Indicators
1. Buzzer
1. Max 232 
1. Serial communication







APPLICATIONS:

1. Industrial
1. Banks
1. Home appliances

ADVANTAGES: 
1.  Low Cost 
1. Automated operation
1. low power consumption
1. very flexible 
1. Easy To Manufacture.















Further details contact: a vinay 9030333433, 08772261612
email: takeoffstudentprojects@gmail.com | www.takeoffprojects.com
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