
DESIGN AND DEVELOPMENT OF EMBEDDED MEDIA PLAYER USING S3C2440 AND SDL​_FFMPEG
AIM:

The main aim the project is to design “DESIGN AND DEVELOPMENT OF MEDIA PLAYER USING ARM9”.
ABSTRACT:
The embedded multi-media terminal was designed and developed, using SAMSUNG Corporation's S3C2440 chip as core processor.
Multi-media terminal is capable of storing and playing digital media such as audio, images, video, documents, etc. the data is typically stored on a hard drive, micro drive, or flash memory. 
Our Embedded project is to design and develop a low cost feature which is based on embedded platform for audio and video player and other GUI interface. The product is be used as a remote multi-media communications platform for multiple applications areas. 
Our Embedded system uses ARM9 micro controller which is 32 bit controller. The audio and video files are given to the controller through Pen drive or SD Card. The controller process the information and given to Audio and video display unit. The touch screen acts as both video and audio display unit as well as it can also be used for selecting files and as controlling player.
The main aim of our project is to take the data from the pen drive through USB device or from the SD card. Our system is designed by implementing display driver, USB drives and audio and video drivers for developing it as a media player.
Here we are going to use S3C2440 based micro controller to implement this project. 
BLOCK DIAGRAM:
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IMPLEMENTATION:
OPERATING SYSTEM:  Linux Ported into ARM controller.

TARGET DEVICE:   S3C2440 (Friendly ARM9).

APPLICATION LANGUAGE:   ‘C’/ ‘C++’.
APPLICATIONS:  Can be used as playing audio and video files and displaying the images.

REFERENCE: 
1. The 8051 micro controller and embedded systems by Mazidi. 
2. Datasheets and the user manuals of S3C2440.
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