Implementation of Obstacle Avoidance and ZigBee Control Functions for Omni Directional Mobile Robot 
ABSTRACT:
 
Mobile robots perform various ways of tasks to serve humans such as home robot, inspection robot, security robot, school education robot, rehabilitation robot, and so on. The conventional mobile robots have used front-steering and rear- wheel driving mechanism to response all needed robot obvious motions, but the motion restriction is a major problem in the use of such mechanism. The omni directional configuration is a most suggested mechanism for mobile robot, which to have the capability of changing directions within the limited space in the indoor environment.
             The ODMR (Omni directional mobile robot) uses IR sensor to sense the obstacle and send the obstacle distance signal to embedded controller. The embedded controller receives these obstacle detecting signals and then calculates the control signals to drive the motors to change the direction for the robot. ZigBee interface is also provided on the robot to give some control signals from the Personal computer attached with ZigBee enabled circuit. Using this ZigBee interface we can control the direction, speed for the robot.
   In our proposed robot we are using microcontroller to control the IR sensor and robot Motors. Robot can move in any direction. But when any obstacle comes in front of the robot, IR sensor senses that obstacle and send appropriate signal to the microcontroller. Once the microcontroller receives IR signal then it itself having program to give necessary control instructions to motor or it will send that IR detection signals to personal computer using wireless link of Zigbee. PC having programmed that will provide appropriate control signals to microcontroller using Zigbee wireless link. After receiving this signal at microcontroller, it direct that signal to the motor. 
In this project we going use microcontroller, which the current dominant microcontroller in mobile based products and software development Tool as Keil, flash magic for loading hex file in to the microcontroller

BLOCK DIAGRAM:
TRANSMITTER:

RECEIVER:


SOFTWARE: Embedded ‘C’

TOOLS: Keil, Flash magic.

TARGET DEVICE: Microcontroller.

APPLICATIONS: we can use these pc based robots in industries where it is                      impossible to the human beings

ADVANTAGES: Low cost, wireless and PC controlling.

    REFERENCE: The 8051 micro controller and embedded systems by Mazidi 
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