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			RFID BASED PAID CAR PARKING
ABSTRACT:
RFID based car parking uses a microcontroller along with sensing circuits monitoring entry and exit of cars. The car owners are allowed an entry only when their RFID card is swiped .The amount in the card automatically gets reduced with a display indication besides indicating the available number of parking. For loading the amount 2 push buttons are used SW1 for Rs500 and SW2 for 300.Example is shown for 2 cards but it can be extended to many numbers. An H-bridge arrangement operates the entry and exit boom motors operating clockwise and anticlockwise for opening and closing. A buzzer sound comes while the card is swiped. Upon every entry of a car the parking availability gets reduced by one number while every exit the number increases. A standard power supply is used. A LCD displays the status. A switch is used in place of RFID for minimizing the project cost.
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HARDWARE REQUIREMENT:
1. Buzzer
2. Rfid Reader
3. Rfid Tag
4. Dc Motor
5. Micro Controller
6. Lcd Display
SOFTWARE REQUIREMENTS:
· Keil compiler,
· Languages: Embedded C or Assembly                                   

ADVANTAGES:
· Highly sensitive      
· Visual identification with LED 
· Low cost and reliable circuit 
· Sensitivity can be adjusted 

Applications:
· Parking Places
· Toll Gates
· Shoping Malls
Further Details Contact: A Vinay 9030333433, 08772261612
Email: takeoffstudentprojects@gmail.com | www.takeoffprojects.com
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