
MULTI-ROBOTS COMMUNICATION SYSTEM BASED ON MULTI NODE WIRELESS ZIGBEE NETWORK
ABSTRACT:
The wireless communication technologies are rapidly spreading to many new areas, including the automation and the importance of the use of wireless technologies in the data acquisition, building control, monitoring systems and automation of manufacturing processes will grow. Intelligent mobile robots and cooperative multi- agent robotic systems can be very efficient tools to speed up search and research operations in remote areas. 
Robots are also useful to do jobs in areas and in situations that are hazardous for human. They can go anywhere that is not reachable my humans and can go into gaps and move trough small holes that are impossible for humans and even trained dogs. 
Our preliminary aim in this project is to build an multi robot communication, which could be able to slave robot follow the master robot, intelligent can create only master robot than control remain slave robots, and what is the obstacle in present master robot can direction and same command can pass through zigbee to slave robot in this way we can speed up the work process in industrial management by zigbee communication. 

This project uses regulated 5V, 750mA power supply. 7805 three terminal voltage regulator is used for voltage regulation. Bridge type full wave rectifier is used to rectify the ac output of secondary of 230/18V step down transformer.









BLOCK DIAGRAM: MATER ROBOT
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BLOCK DIAGRAM: SLAVE ROBOT
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HARDWARE REQUIREMENTS:
        
HARDWARE REQUIREMENTS:
       TRANSMITTER:
· Microcontroller
· Power supply
· IR
· Max232
· 12v Battery
· Zigbee
· Robot platform
       RECEIVER:
· Microcontroller
· Power supply
· Max232
· Zigbee
· Robot platform
· 12v Battery
SOFTWARE REQUIREMENTS:
· KEIL software
· RIDE Software






ADVANTAGES:
· More useful in remote areas
· Firing events more help full to save
· Easily operated

APPLICATIONS:
· Military applications
· Landmine detection
· Firing situations



Further Details Contact: A Vinay 9030333433, 08772261612
Email: takeoffstudentprojects@gmail.com | www.takeoffprojects.com
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